{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["建筑工程","临时工程"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"建筑工程","index":0,"n_rows":139,"n_cols":6,"rows_kept":139,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
[" 西峡县丹水河七峪村至廖坟村段河道治理工程（一期）--K0+000～K5+900（1标）建筑工程量清单"]
["序号","工程或费用名称","单位","数量","单价(元)","合计(万元)"]
["","第一部分  建筑工程","",0,0,{"v":0,"d":"0.00"}]
["壹","第一部分  建筑工程","",0]
["二","防护工程","",0]
["1","桩号K0+000~K0+200左岸格宾石笼护坡","",0]
["1.1","岸坡土方开挖（机械、Ⅳ类土、弃土运2km）","m3",2590.119]
["1.2","格宾石笼护坡（0.3m厚）","m3",429.35]
["1.3","C25砼压顶（0.3×0.5m）","m3",35.2]
["1.4","格宾石笼护脚（0.5m厚）","m3",451.92]
["1.5","护脚土方开挖（机械、Ⅳ类土、用于土方回填）","m3",93.22]
["1.6","护脚土方开挖（机械、Ⅳ类土、弃土运2km）","m3",248.03]
["1.7","护脚土方回填（机械、Ⅳ类土）","m3",78.75]
["1.8","闭孔低发泡沫塑料板伸缩缝","m2",7.09]
["1.9","普通标准钢模板","m2",234.61]
["1.10","反滤土工布（300g/m2）","m2",2171.33]
["2","桩号K0+000~K0+200右岸格宾石笼护坡","",0]
["2.1","岸坡土方开挖（机械、Ⅳ类土、弃土运2km）","m3",671.35]
["2.2","格宾石笼护坡（0.3m厚）","m3",419.99]
["2.3","C25砼压顶（0.3×0.5m）","m3",32.22]
["2.4","格宾石笼护脚（0.5m厚）","m3",422.25]
["2.5","护脚土方开挖（机械、Ⅳ类土、用于土方回填）","m3",93.22]
["2.6","护脚土方开挖（机械、Ⅳ类土、弃土运2km）","m3",169.28]
["2.7","护脚土方回填（机械、Ⅳ类土）","m3",78.75]
["2.8","闭孔低发泡沫塑料板伸缩缝","m2",7.09]
["2.9","普通标准钢模板","m2",234.61]
["2.10","反滤土工布（300g/m2）","m2",2080.63]
["3","K5+140~K5+900左岸格宾石笼护坡","",0]
["3.1","清基（机械、Ⅳ类土、弃土运2km）","m3",2692.05]
["3.2","岸坡土方开挖（机械、Ⅳ类土、用于本段回填）","m3",286.23]
["3.3","岸坡土方开挖（机械、Ⅳ类土、附近取土2km用于岸坡土方回填）","m3",{"v":707.498,"d":"707.50"}]
["3.4","岸坡土方回填（机械、Ⅳ类土料）","m3",4337.13]
["3.5","护脚土方开挖（机械、Ⅳ类土、用于土方回填）","m3",1530.8]
["3.6","护脚土方回填（机械、Ⅳ类土）","m3",315.42]
["3.7","格宾石笼护坡（0.3m厚）","m3",2769.17]
["3.8","C25砼压顶（0.3×0.5）","m3",119.7]
["3.9","格宾石笼护脚（0.5m厚）","m3",1197]
["3.10","撒播草籽护坡","m2",2250.82]
["3.11","普通标准钢模板","m2",468.43]
["3.12","闭孔低发泡沫塑料板伸缩缝","m2",525.47]
["3.13","反滤土工布（300g/m2）","m2",11205.71]
["3.14","砼护坡拆除弃运2km","m3",747.25]
["3.15","砼护脚拆除弃运2km","m3",399]
["4","K5+140~K5+900右岸格宾石笼护坡","",0]
["4.1","清基（机械、Ⅳ类土、弃土运2km）","m3",{"v":2249.407125,"d":"2249.41"}]
["4.2","岸坡土方开挖（机械、Ⅳ类土、用于本段回填）","m3",{"v":242.25468750000002,"d":"242.25"}]
["4.3","岸坡土方开挖（机械、Ⅳ类土、附近取土2km用于岸坡土方回填）","m3",{"v":1993.8497250000003,"d":"1993.85"}]
["4.4","岸坡土方回填（机械、Ⅳ类土）","m3",{"v":2946.7200000000003,"d":"2946.72"}]
["4.5","护脚土方开挖（机械、Ⅳ类土、用于本段回填）","m3",{"v":1568.8181250000002,"d":"1568.82"}]
["4.6","护脚土方回填（机械、Ⅳ类土）","m3",{"v":277.79062500000003,"d":"277.79"}]
["4.7","格宾石笼护坡（0.3m厚）","m3",{"v":2159.3840625000003,"d":"2159.38"}]
["4.8","C25砼压顶（0.3×0.5）","m3",{"v":119.50312500000001,"d":"119.50"}]
["4.9","格宾石笼护脚（0.5m厚）","m3",{"v":1195.03125,"d":"1195.03"}]
["4.10","普通标准钢模板","m2",{"v":428.2497665165792,"d":"428.25"}]
["4.11","闭孔低发泡沫塑料板伸缩缝","m2",{"v":435.9869989597649,"d":"435.99"}]
["4.12","反滤土工布（300g/m2）","m2",9827.02]
["4.13","砼护坡拆除弃运2km","m3",794.98]
["4.14","砼护脚拆除弃运2km","m3",398.34]
["三","建筑物工程","",0]
["1","K0+208漫水桥拆除重建(2跨8米）","",0]
["1.1","漫水桥土方开挖（机械、Ⅳ类土、用于土方回填）","m3",954.62]
["1.2","漫水桥土方开挖（机械、Ⅳ类土、弃土运2km）","m3",149.11]
["1.3","漫水桥土方回填（机械、Ⅳ类土）","m3",809.06]
["1.4","C40钢筋砼现浇板（50cm厚）","m3",41.06]
["1.5","现浇C30钢筋砼台帽（0.3m厚）","m3",5.1]
["1.6","现浇C30钢筋砼背墙（0.7m厚）","m3",3.07]
["1.7","现浇C30钢筋砼桥台挡块（0.15m厚）","m3",0.14]
["1.8","现浇C30钢筋砼中墩盖梁（高1m）","m3",8.11]
["1.9","现浇C30钢筋砼中墩挡块（0.2m厚)","m3",0.13]
["1.10","现浇C30钢筋砼中墩立柱（直径1m）","m3",4.27]
["1.11","现浇C30钢筋砼中墩基础（0.5m厚）","m3",40.04]
["1.12","C30混凝土桥台（1.3m厚）","m3",167.15]
["1.13","现浇C40钢筋砼桥面铺装","m3",9.05]
["1.14","现浇C30钢筋砼防撞护栏","m3",10.752]
["1.15","C30钢筋砼桥头搭板（0.3m厚）","m3",18.9]
["1.16","J75D40伸缩缝","m",10.08]
["1.17","C50钢纤维混凝土","m3",1.52]
["1.18","钢筋制安","t",9.27]
["1.19","普通标准钢模板","m2",695.17]
["1.20","普通曲面模板","m2",22.95]
["1.21","C25砼路面恢复（0.18m厚）","m2",63]
["1.22","碎石垫层","m3",6.3]
["1.23","标识牌","个",1]
["1.24","老漫水桥砼拆除（弃运2km）","m3",188.27]
["1.25","C20砼路面拆除（弃运2km）","m3",11.34]
["1.26","C25砼垫层（0.1m厚）","m3",21.06]
["1.27","桥上下游护坡（各长10m）","",0]
["1.27.1","C25砼压顶","m3",6.3]
["1.27.2","护坡土方开挖（机械、Ⅳ类土、用于土方回填）","m3",23.6]
["1.27.3","护坡土方开挖（机械、Ⅳ类土、弃土运2km）","m3",319.35]
["1.27.4","护坡土方回填（机械、Ⅳ类土）","m3",20.37]
["1.27.5","格宾石笼护坡（0.3m厚）","m3",75.6]
["1.27.6","格宾石笼护脚（0.5m厚）","m3",63]
["1.27.7","反滤土工布（300g/m2）","m2",384.93]
["1.27.8","普通标准钢模板","m2",42]
["1.27.9","闭孔低发泡沫塑料板伸缩缝","m2",0.32]
["2","K3+485漫水桥拆除重建(2跨10米）","",0]
["2.1","漫水桥土方开挖（机械、Ⅳ类土、用于土方回填）","m3",826]
["2.2","漫水桥土方开挖（机械、Ⅳ类土、弃土运2km）","m3",127]
["2.3","漫水桥土方回填（机械、Ⅳ类土）","m3",700.4]
["2.4","C40钢筋砼现浇板（50cm厚）","m3",51.35]
["2.5","现浇C30钢筋砼台帽（0.3m厚）","m3",5.1]
["2.6","现浇C30钢筋砼背墙（0.7m厚）","m3",3.07]
["2.7","现浇C30钢筋砼桥台挡块（0.15m厚）","m3",0.14]
["2.8","现浇C30钢筋砼中墩盖梁（高1m）","m3",8.11]
["2.9","现浇C30钢筋砼中墩挡块（0.2m厚)","m3",0.13]
["2.10","现浇C30钢筋砼中墩立柱（直径1m）","m3",8.23]
["2.11","现浇C30钢筋砼中墩基础（0.5m厚）","m3",40.04]
["2.12","C30混凝土桥台（1.3m厚）","m3",205.99]
["2.13","现浇C40钢筋砼桥面铺装","m3",9.05]
["2.14","现浇C30钢筋砼防撞护栏","m3",13.44]
["2.15","C30钢筋砼桥头搭板（0.3m厚）","m3",18.9]
["2.16","J75D40伸缩缝","m",10.08]
["2.17","C50钢纤维混凝土","m3",1.52]
["2.18","钢筋制安","t",10.17]
["2.19","普通标准钢模板","m2",737.29]
["2.20","普通曲面模板","m2",32.9]
["2.21","C25砼路面恢复（0.18m厚）","m2",147]
["2.22","碎石垫层","m3",14.7]
["2.23","标识牌","个",1]
["2.24","老漫水桥砼拆除（弃运2km）","m3",276.19]
["2.25","C20砼路面拆除（弃运2km）","m3",12.1]
["2.26","C25砼垫层（0.1m厚）","m3",21.31]
["2.27","桥上下游护坡（各长10m）","",0]
["2.27.1","护坡土方开挖（机械、Ⅳ类土、用于土方回填）","m3",18.88]
["2.27.2","护坡土方开挖（机械、Ⅳ类土、弃土运2km）","m3",200.99]
["2.27.3","护坡土方回填（机械、Ⅳ类土）","m3",15.96]
["2.27.4","C25砼压顶","m3",6.3]
["2.27.5","格宾石笼护坡（0.3m厚）","m3",113.4]
["2.27.6","格宾石笼护脚（0.5m厚）","m3",63]
["2.27.7","反滤土工布（300g/m2）","m2",504]
["2.27.8","普通标准钢模板","m2",42]
["2.27.9","闭孔低发泡沫塑料板伸缩缝","m2",0.32]
["3","漫水桥拆除工程","",0]
["3.1","K1+425漫水桥砼拆除(弃运2km)","m3",202.55]
["3.2","K2+745漫水桥砼拆除(弃运2km)","m3",180.02]
["3.3","K2+223溢流堰砼拆除(弃运2km)","m3",86.88]
["3.4","K3+375溢流堰砼拆除(弃运2km)","m3",122.28]
["3.5","K3+995溢流堰砼拆除(弃运2km)","m3",188.47]

{"sheet":"临时工程","index":1,"n_rows":21,"n_cols":6,"rows_kept":21,"merged":[[0,0,0,5]],"flags":["formulas_cached_only"]}
[" 西峡县丹水河七峪村至廖坟村段河道治理工程（一期）--K0+000～K5+900（1标）临时工程量清单"]
["序号","工程或费用名称","单位","数量","单价(元)","合计(万元)"]
["","第四部分  施工临时工程","",0,0,{"v":0,"d":"0.00"}]
["肆","第四部分  施工临时工程","",0]
["一","导流工程","",0]
["1","K0+208漫水桥拆除重建(2跨8米）","",0]
["1.1","围堰土方填筑（利用开挖料）","m3",297.82]
["1.2","围堰土方拆除（弃土运2km）","m3",351.4276]
["1.3","DN1000预制砼涵管","m",46]
["2","K3+485漫水桥拆除重建(2跨10米）","",0]
["2.1","围堰土方填筑（利用开挖料）","m3",578.63]
["2.2","围堰土方拆除（弃土运2km）","m3",682.7834]
["2.3","DN1000预制砼涵管","m",92]
["二","施工交通工程","",0]
["1","临时道路基础","m2",5550]
["2","泥结碎石路面","m2",5550]
["三","施工场外供电工程","",0]
["四","施工房屋建筑工程","",0]
["1","施工仓库","m2",200]
["2","办公、生活及文化福利建筑","%",1.5]
["五","其他临时工程","%",1]